<?xml version="1.0"?>
<fc:FIRMWARE-CONFIG xmlns:std="http://www.eberspaecher.com/electronics/xml/fcm/standardsignals" xmlns:secoc="http://www.eberspaecher.com/electronics/xml/fcm/securedOnboardCommunication" xmlns:gv="http://www.eberspaecher.com/electronics/xml/fcm/globalvariables" xmlns:dv="http://www.eberspaecher.com/electronics/xml/fcm/fcmDefaultValues" xmlns:gts="http://www.eberspaecher.com/electronics/xml/fcm/globaltimesync" xmlns:vsm="http://www.eberspaecher.com/electronics/xml/fcm/vsm" xmlns:tp="http://www.eberspaecher.com/electronics/xml/fcm/transportProtocols" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:cecu="http://www.eberspaecher.com/electronics/xml/fcm/fcmAdditionalEcus" xmlns:mn="http://www.eberspaecher.com/electronics/xml/fcm/fcmManipulation" xmlns:log="http://www.eberspaecher.com/electronics/xml/fcm/logging" xmlns:gw="http://www.eberspaecher.com/electronics/xml/fcm/gateway" xmlns:file="http://www.eberspaecher.com/electronics/xml/fcm/userfiles" xmlns:uf="http://www.eberspaecher.com/electronics/xml/fcm/userfunctions" xmlns:fca="http://www.eberspaecher.com/electronics/xml/fcm/Analyzer" xmlns:txb="http://www.eberspaecher.com/electronics/xml/fcm/fcmTxBehavior" xmlns:e2e="http://www.eberspaecher.com/electronics/xml/fcm/e2e" VERSION="8.2.3.0" xmlns:fc="http://www.eberspaecher.com/electronics/xml/fcm">
  <fc:PROJECT>
    <fc:SHORT-NAME>FlexDevice_S</fc:SHORT-NAME>
    <fc:LONG-NAME />
    <fc:DESC />
    <fc:CREATE-VERSION>
      <fc:VERSION>5.3.5.0</fc:VERSION>
      <fc:DATE>2021-07-19T18:07:16.8223346+02:00</fc:DATE>
    </fc:CREATE-VERSION>
    <fc:SAVE-VERSION>
      <fc:VERSION>5.3.5.0</fc:VERSION>
      <fc:DATE>2021-09-21T11:50:03.3227229+02:00</fc:DATE>
      <fc:BUILD-ITEMS>None</fc:BUILD-ITEMS>
    </fc:SAVE-VERSION>
    <fc:LAST-COMPILE>
      <fc:VERSION>5.3.5.0</fc:VERSION>
      <fc:DATE>2021-09-21T11:49:45.5763223</fc:DATE>
      <fc:TIMESTAMP>637678217855763223</fc:TIMESTAMP>
      <fc:S19-HASH>8A37D222A259D83A5A53330C7C29D747</fc:S19-HASH>
      <fc:AUTOCODER-VERSION>Ebel.Autocoder, Version=8.2.4.0, Culture=neutral, PublicKeyToken=null</fc:AUTOCODER-VERSION>
    </fc:LAST-COMPILE>
  </fc:PROJECT>
  <fc:APPLICATION>
    <fc:SOURCES>
      <fc:SOURCE xsi:type="std:SOURCE-TYPE" GUID="f0b3049d-0603-4d20-818c-59c1549bda7c">
        <fc:SHORT-NAME>RestBusSimulation_at_CAN1</fc:SHORT-NAME>
        <fc:FORMAT>FIBEX</fc:FORMAT>
        <fc:VERSION>4.1.1</fc:VERSION>
        <fc:PATH>.\CAN1\Tutorials_v002.xml</fc:PATH>
        <fc:CLUSTER ID-REF="clusterCAN" />
        <fc:CHANNELS>
          <fc:CHANNEL ID-REF="CANc" />
        </fc:CHANNELS>
        <fc:SPEED>500000</fc:SPEED>
        <fc:BUS-ID>CAN1</fc:BUS-ID>
        <fc:INTERNAL-BUS-ID>CAN10</fc:INTERNAL-BUS-ID>
        <fc:REAL-ECUS />
        <fc:SIM-ECUS>
          <fc:SIM-ECU ID-REF="ecu_1" />
          <fc:SIM-ECU ID-REF="ecu_6" />
        </fc:SIM-ECUS>
        <fc:IGNORED-ECUS />
        <fc:ADDITIONAL-FRAMES>
          <fc:ADDITIONAL-FRAME ID-REF="frtr_5" DIRECTION="transmit" USAGE="RBS" />
          <fc:ADDITIONAL-FRAME ID-REF="frtr_4" DIRECTION="transmit" USAGE="RBS" />
        </fc:ADDITIONAL-FRAMES>
        <fc:SERVICES>
          <fc:PROVIDED-SERVICES />
          <fc:CONSUMED-SERVICES />
        </fc:SERVICES>
        <fc:BLOCK-FRAMES />
        <fc:SYNC-STRATEGY>EnsureStartupStrategy</fc:SYNC-STRATEGY>
        <fc:STATIC-ARP-ENTRIES />
        <fc:PROPERTIES>
          <fc:PROPERTY NAME="Count" VALUE="1" SECTION="Bus.Controller" />
          <fc:PROPERTY NAME="UseAnalyzing" VALUE="true" SECTION="General" />
          <fc:PROPERTY NAME="BusType" VALUE="CAN-HS" SECTION="General" />
          <fc:PROPERTY NAME="MinimumCyclicTiming" VALUE="5" SECTION="Bus.Timing" />
        </fc:PROPERTIES>
        <std:STANDARD-SIGNALS />
      </fc:SOURCE>
      <fc:SOURCE xsi:type="txb:SOURCE-TYPE" GUID="8c52a3f5-2505-484a-94fa-bfe5d7b683bb">
        <fc:FORMAT>XML</fc:FORMAT>
        <fc:VERSION>2.0.1.0</fc:VERSION>
        <fc:PATH>TxBehavior.xml</fc:PATH>
      </fc:SOURCE>
      <fc:SOURCE xsi:type="uf:SOURCE-TYPE" GUID="cb27b2f4-7d10-4015-8d77-6134db6e39e5">
        <fc:SHORT-NAME>UserFunctionSource</fc:SHORT-NAME>
        <fc:FORMAT>C</fc:FORMAT>
        <fc:PATH />
        <uf:FUNCTIONS>
          <uf:TX-FUNCTIONS>
            <uf:TX-FUNCTION IS-ACTIVE="true">
              <uf:INPUT-PARAMETERS>
                <uf:PARAMETER TYPE="SIGNAL">
                  <uf:CODE-NAME>Drive_Speed</uf:CODE-NAME>
                  <uf:DATATYPE>uint8</uf:DATATYPE>
                  <uf:BUS-ID>CAN1</uf:BUS-ID>
                  <uf:CHANNEL>CANc</uf:CHANNEL>
                  <uf:REF>sigi_5_3</uf:REF>
                  <uf:PARENTREF>frtr_5</uf:PARENTREF>
                  <uf:METHODTYPE>InternalValue</uf:METHODTYPE>
                </uf:PARAMETER>
              </uf:INPUT-PARAMETERS>
              <uf:OUTPUT-PARAMETERS>
                <uf:PARAMETER TYPE="SIGNAL">
                  <uf:CODE-NAME>Drive_Speed</uf:CODE-NAME>
                  <uf:DATATYPE>uint8</uf:DATATYPE>
                  <uf:BUS-ID>CAN1</uf:BUS-ID>
                  <uf:CHANNEL>CANc</uf:CHANNEL>
                  <uf:REF>sigi_5_3</uf:REF>
                  <uf:PARENTREF>frtr_5</uf:PARENTREF>
                  <uf:METHODTYPE>InternalValue</uf:METHODTYPE>
                </uf:PARAMETER>
              </uf:OUTPUT-PARAMETERS>
              <uf:RETURN-VALUE>
                <uf:VALUE>1</uf:VALUE>
                <uf:TYPE>uint8</uf:TYPE>
              </uf:RETURN-VALUE>
              <uf:CODE><![CDATA[
	/*
	To disable or enable the standard signal calculation, please use the
	parameters of the user function above.
	
	0 = disable calculation
	1 = enable calculation
	*/
	
			u08 Drive_Speed = SODA_get_SIGNAL_CAN1_sigi_5_3();
	Drive_Speed++;
	SODA_set_SIGNAL_CAN1_sigi_5_3(Drive_Speed);
	/* Write your code here... */
	
	return 1; /*0 = disables frame transmission; 1 = enables frame transmission*/
]]></uf:CODE>
              <uf:NAME>CAN1_Frame_Drive_frame_OnTx</uf:NAME>
              <uf:CHANNEL-ID>CANc</uf:CHANNEL-ID>
              <uf:FRAME-TRIGGERING-REF>frtr_5</uf:FRAME-TRIGGERING-REF>
              <uf:BUS-ID>CAN1</uf:BUS-ID>
            </uf:TX-FUNCTION>
            <uf:TX-FUNCTION IS-ACTIVE="true">
              <uf:INPUT-PARAMETERS>
                <uf:PARAMETER TYPE="SIGNAL">
                  <uf:CODE-NAME>Engine_Speed</uf:CODE-NAME>
                  <uf:DATATYPE>uint8</uf:DATATYPE>
                  <uf:BUS-ID>CAN1</uf:BUS-ID>
                  <uf:CHANNEL>CANc</uf:CHANNEL>
                  <uf:REF>sigi_4_3</uf:REF>
                  <uf:PARENTREF>frtr_4</uf:PARENTREF>
                  <uf:METHODTYPE>InternalValue</uf:METHODTYPE>
                </uf:PARAMETER>
                <uf:PARAMETER TYPE="SIGNAL">
                  <uf:CODE-NAME>Engine_Temperature</uf:CODE-NAME>
                  <uf:DATATYPE>uint8</uf:DATATYPE>
                  <uf:BUS-ID>CAN1</uf:BUS-ID>
                  <uf:CHANNEL>CANc</uf:CHANNEL>
                  <uf:REF>sigi_4_4</uf:REF>
                  <uf:PARENTREF>frtr_4</uf:PARENTREF>
                  <uf:METHODTYPE>InternalValue</uf:METHODTYPE>
                </uf:PARAMETER>
              </uf:INPUT-PARAMETERS>
              <uf:OUTPUT-PARAMETERS>
                <uf:PARAMETER TYPE="SIGNAL">
                  <uf:CODE-NAME>Engine_Speed</uf:CODE-NAME>
                  <uf:DATATYPE>uint8</uf:DATATYPE>
                  <uf:BUS-ID>CAN1</uf:BUS-ID>
                  <uf:CHANNEL>CANc</uf:CHANNEL>
                  <uf:REF>sigi_4_3</uf:REF>
                  <uf:PARENTREF>frtr_4</uf:PARENTREF>
                  <uf:METHODTYPE>InternalValue</uf:METHODTYPE>
                </uf:PARAMETER>
                <uf:PARAMETER TYPE="SIGNAL">
                  <uf:CODE-NAME>Engine_Temperature</uf:CODE-NAME>
                  <uf:DATATYPE>uint8</uf:DATATYPE>
                  <uf:BUS-ID>CAN1</uf:BUS-ID>
                  <uf:CHANNEL>CANc</uf:CHANNEL>
                  <uf:REF>sigi_4_4</uf:REF>
                  <uf:PARENTREF>frtr_4</uf:PARENTREF>
                  <uf:METHODTYPE>InternalValue</uf:METHODTYPE>
                </uf:PARAMETER>
              </uf:OUTPUT-PARAMETERS>
              <uf:RETURN-VALUE>
                <uf:VALUE>1</uf:VALUE>
                <uf:TYPE>uint8</uf:TYPE>
              </uf:RETURN-VALUE>
              <uf:CODE><![CDATA[
	/*
	To disable or enable the standard signal calculation, please use the
	parameters of the user function above.
	
	0 = disable calculation
	1 = enable calculation
	*/
	
		u08 Engine_Speed = SODA_get_SIGNAL_CAN1_sigi_4_3();
	Engine_Speed++;
	SODA_set_SIGNAL_CAN1_sigi_4_3(Engine_Speed);

	
	/* Signal CAN1.Engine_frame.Engine_pdu.Engine_Temperature */
	/* Linear compumethod:(Vn0:0 Vn1=1 Vd0=1) */
	
	u08 Engine_Temperature = SODA_get_SIGNAL_CAN1_sigi_4_4();

	if(Engine_Temperature == 90)
	{
		SODA_set_SIGNAL_CAN1_sigi_4_4(90);
	}
	else 
	{
		Engine_Temperature++;
		SODA_set_SIGNAL_CAN1_sigi_4_4(Engine_Temperature);
	}
	
	/* Write your code here... */
	
	return 1; /*0 = disables frame transmission; 1 = enables frame transmission*/
]]></uf:CODE>
              <uf:NAME>CAN1_Frame_Engine_frame_OnTx</uf:NAME>
              <uf:CHANNEL-ID>CANc</uf:CHANNEL-ID>
              <uf:FRAME-TRIGGERING-REF>frtr_4</uf:FRAME-TRIGGERING-REF>
              <uf:BUS-ID>CAN1</uf:BUS-ID>
            </uf:TX-FUNCTION>
          </uf:TX-FUNCTIONS>
        </uf:FUNCTIONS>
      </fc:SOURCE>
      <fc:SOURCE xsi:type="fca:SOURCE-TYPE" GUID="054537f3-0c85-4f71-9355-7c90958ffca5">
        <fc:SHORT-NAME>FlexConfigAnalyzer</fc:SHORT-NAME>
        <fc:FORMAT>XML</fc:FORMAT>
        <fc:VERSION>2.0.0.0</fc:VERSION>
        <fc:PATH>Analyzer.fca</fc:PATH>
      </fc:SOURCE>
      <fc:SOURCE xsi:type="std:SOURCE-TYPE" GUID="e3bc1d45-0352-40a4-a7a5-a02d0c008745">
        <fc:SHORT-NAME>Added_Over_Analyzer</fc:SHORT-NAME>
        <fc:FORMAT>Not_Specified</fc:FORMAT>
        <fc:VERSION />
        <fc:PATH />
        <fc:CLUSTER ID-REF="" />
        <fc:CHANNELS />
        <fc:SPEED>100000000</fc:SPEED>
        <fc:BUS-ID>ETH1</fc:BUS-ID>
        <fc:INTERNAL-BUS-ID>ETH3</fc:INTERNAL-BUS-ID>
        <fc:REAL-ECUS />
        <fc:SIM-ECUS />
        <fc:IGNORED-ECUS />
        <fc:ADDITIONAL-FRAMES />
        <fc:BLOCK-FRAMES />
        <fc:SYNC-STRATEGY>EnsureStartupStrategy</fc:SYNC-STRATEGY>
        <fc:STATIC-ARP-ENTRIES />
        <fc:PROPERTIES>
          <fc:PROPERTY NAME="Count" VALUE="1" SECTION="Bus.Controller" />
          <fc:PROPERTY NAME="UseAnalyzing" VALUE="true" SECTION="General" />
          <fc:PROPERTY NAME="BusType" VALUE="BROADR_REACH" SECTION="General" />
          <fc:PROPERTY NAME="TransceiverOption" VALUE="100Base-T1 Slave" SECTION="Bus.Ethernet" />
          <fc:PROPERTY NAME="MaxContainerLength" VALUE="1454" SECTION="Bus.Ethernet" />
          <fc:PROPERTY NAME="MaxContainerLengthTcp" VALUE="31724" SECTION="Bus.Ethernet" />
          <fc:PROPERTY NAME="IpAddress" VALUE="10.0.0.11" SECTION="Bus.Ethernet.FallbackIpSetting" />
          <fc:PROPERTY NAME="SubnetMask" VALUE="255.255.0.0" SECTION="Bus.Ethernet.FallbackIpSetting" />
          <fc:PROPERTY NAME="DefaultGateway" VALUE="10.0.0.1" SECTION="Bus.Ethernet.FallbackIpSetting" />
          <fc:PROPERTY NAME="MacAddress" SECTION="Bus.Ethernet.FallbackIpSetting" />
          <fc:PROPERTY NAME="SourcePort" VALUE="30491" SECTION="Bus.Ethernet.FallbackIpSetting" />
          <fc:PROPERTY NAME="DestinationPort" VALUE="30491" SECTION="Bus.Ethernet.FallbackIpSetting" />
          <fc:PROPERTY NAME="Ipv6Address" VALUE="fc00:0000:0000:0:0000:0000:1:0001" SECTION="Bus.Ethernet.FallbackIpSetting" />
          <fc:PROPERTY NAME="Ipv6PrefixLength" VALUE="64" SECTION="Bus.Ethernet.FallbackIpSetting" />
        </fc:PROPERTIES>
        <std:STANDARD-SIGNALS />
      </fc:SOURCE>
      <fc:SOURCE xsi:type="std:SOURCE-TYPE" GUID="cf56016a-e7f8-403c-9901-84c1e79a0997">
        <fc:SHORT-NAME>Added_Over_Analyzer</fc:SHORT-NAME>
        <fc:FORMAT>Not_Specified</fc:FORMAT>
        <fc:VERSION />
        <fc:PATH />
        <fc:CLUSTER ID-REF="" />
        <fc:CHANNELS />
        <fc:SPEED>500000</fc:SPEED>
        <fc:BUS-ID>CAN2</fc:BUS-ID>
        <fc:INTERNAL-BUS-ID>CAN_FD7</fc:INTERNAL-BUS-ID>
        <fc:REAL-ECUS />
        <fc:SIM-ECUS />
        <fc:IGNORED-ECUS />
        <fc:ADDITIONAL-FRAMES />
        <fc:BLOCK-FRAMES />
        <fc:SYNC-STRATEGY>EnsureStartupStrategy</fc:SYNC-STRATEGY>
        <fc:STATIC-ARP-ENTRIES />
        <fc:PROPERTIES>
          <fc:PROPERTY NAME="Count" VALUE="1" SECTION="Bus.Controller" />
          <fc:PROPERTY NAME="UseAnalyzing" VALUE="true" SECTION="General" />
          <fc:PROPERTY NAME="BusType" VALUE="CAN-FD" SECTION="General" />
          <fc:PROPERTY NAME="CanFdSpeed" VALUE="500000" SECTION="Bus.CanFd" />
          <fc:PROPERTY NAME="Protocol" VALUE="ISO11898 - 1" SECTION="Bus.CanFd" />
        </fc:PROPERTIES>
        <std:STANDARD-SIGNALS />
      </fc:SOURCE>
      <fc:SOURCE xsi:type="std:SOURCE-TYPE" GUID="b9c11fb4-5828-4441-8a83-36eef3d9ed3f">
        <fc:SHORT-NAME>Added_Over_Analyzer</fc:SHORT-NAME>
        <fc:FORMAT>Not_Specified</fc:FORMAT>
        <fc:VERSION />
        <fc:PATH />
        <fc:CLUSTER ID-REF="" />
        <fc:CHANNELS />
        <fc:SPEED>500000</fc:SPEED>
        <fc:BUS-ID>CAN3</fc:BUS-ID>
        <fc:INTERNAL-BUS-ID>CAN_FD8</fc:INTERNAL-BUS-ID>
        <fc:REAL-ECUS />
        <fc:SIM-ECUS />
        <fc:IGNORED-ECUS />
        <fc:ADDITIONAL-FRAMES />
        <fc:BLOCK-FRAMES />
        <fc:SYNC-STRATEGY>EnsureStartupStrategy</fc:SYNC-STRATEGY>
        <fc:STATIC-ARP-ENTRIES />
        <fc:PROPERTIES>
          <fc:PROPERTY NAME="Count" VALUE="1" SECTION="Bus.Controller" />
          <fc:PROPERTY NAME="UseAnalyzing" VALUE="true" SECTION="General" />
          <fc:PROPERTY NAME="BusType" VALUE="CAN-FD" SECTION="General" />
          <fc:PROPERTY NAME="CanFdSpeed" VALUE="500000" SECTION="Bus.CanFd" />
          <fc:PROPERTY NAME="Protocol" VALUE="ISO11898 - 1" SECTION="Bus.CanFd" />
        </fc:PROPERTIES>
        <std:STANDARD-SIGNALS />
      </fc:SOURCE>
      <fc:SOURCE xsi:type="std:SOURCE-TYPE" GUID="9521de06-6208-449c-be7f-4eaad536a885">
        <fc:SHORT-NAME>Added_Over_Analyzer</fc:SHORT-NAME>
        <fc:FORMAT>Not_Specified</fc:FORMAT>
        <fc:VERSION />
        <fc:PATH />
        <fc:CLUSTER ID-REF="" />
        <fc:CHANNELS />
        <fc:SPEED>500000</fc:SPEED>
        <fc:BUS-ID>CAN4</fc:BUS-ID>
        <fc:INTERNAL-BUS-ID>CAN9</fc:INTERNAL-BUS-ID>
        <fc:REAL-ECUS />
        <fc:SIM-ECUS />
        <fc:IGNORED-ECUS />
        <fc:ADDITIONAL-FRAMES />
        <fc:BLOCK-FRAMES />
        <fc:SYNC-STRATEGY>EnsureStartupStrategy</fc:SYNC-STRATEGY>
        <fc:STATIC-ARP-ENTRIES />
        <fc:PROPERTIES>
          <fc:PROPERTY NAME="Count" VALUE="1" SECTION="Bus.Controller" />
          <fc:PROPERTY NAME="UseAnalyzing" VALUE="true" SECTION="General" />
          <fc:PROPERTY NAME="BusType" VALUE="CAN-HS" SECTION="General" />
        </fc:PROPERTIES>
        <std:STANDARD-SIGNALS />
      </fc:SOURCE>
    </fc:SOURCES>
    <fc:SETTINGS>
      <fc:GLOBALDEFINES>
        <fc:GLOBALDEFINE>
          <fc:SYMBOL>START_IMMEDIATELY</fc:SYMBOL>
        </fc:GLOBALDEFINE>
      </fc:GLOBALDEFINES>
      <fc:IP-SETTINGS>
        <fc:NETMASK>255.255.255.0</fc:NETMASK>
        <fc:IP-ADDRESS>192.168.1.15</fc:IP-ADDRESS>
        <fc:STANDARDGATEWAY>192.168.1.1</fc:STANDARDGATEWAY>
      </fc:IP-SETTINGS>
      <fc:DEVICE>
        <fc:TYPE>FlexDevice-S</fc:TYPE>
        <fc:PROPERTIES>
          <fc:PROPERTY NAME="DEVICE-REVISION" VALUE="0A01-01" />
          <fc:PROPERTY NAME="DEVICE-VARIANT" VALUE="0x000000B0" />
          <fc:PROPERTY NAME="FPGA-IMAGE 1" VALUE="0xB0" />
          <fc:PROPERTY NAME="FPGA-IMAGE-VERSION 1" VALUE="1.0.9.5" />
          <fc:PROPERTY NAME="DEVICE-PLATFORM" VALUE="DevicePlatformFlexMod" />
          <fc:PROPERTY NAME="IS-HIGH-LOW-BYTE-ORDER" VALUE="false" />
          <fc:PROPERTY NAME="OS-VARIANT" VALUE="ARM EABI HF GCC FPU" />
        </fc:PROPERTIES>
      </fc:DEVICE>
      <fc:ADDITIONALS>
        <fc:ADDITIONAL>
          <fc:NAME>GUI.CurrentBuildNumber</fc:NAME>
          <fc:VALUE>0006</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>SyncFrameStrategy</fc:NAME>
          <fc:VALUE>EnsureStartupStrategy</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>ContainerPduFifoCount</fc:NAME>
          <fc:VALUE>100</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>CreateSignalPhysicalFunctions</fc:NAME>
          <fc:VALUE>false</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>FifoCount</fc:NAME>
          <fc:VALUE>10</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>FifoCriticalLevel</fc:NAME>
          <fc:VALUE>6</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>UserString</fc:NAME>
          <fc:VALUE>#BNr            </fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>FR_FRAME_INIT_VALUE</fc:NAME>
          <fc:VALUE>0xFFFF</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>CAN_FRAME_INIT_VALUE</fc:NAME>
          <fc:VALUE>0xFF</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>PDU_INIT_VALUE</fc:NAME>
          <fc:VALUE>0xFF</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>secOC-DefaultAuthenticatorValue</fc:NAME>
          <fc:VALUE>0xFFFFFFFFFFFFFFFFFFFFFFFFFFFFFFFF</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>secOC-DefaultFreshnessValue</fc:NAME>
          <fc:VALUE>0xFFFFFFFFFFFFFFFF</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>GatewayViewMode</fc:NAME>
          <fc:VALUE>1</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>CanAttachFpgaToProject</fc:NAME>
          <fc:VALUE>true</fc:VALUE>
        </fc:ADDITIONAL>
        <fc:ADDITIONAL>
          <fc:NAME>RouteSecOCTrailer</fc:NAME>
          <fc:VALUE>false</fc:VALUE>
        </fc:ADDITIONAL>
      </fc:ADDITIONALS>
    </fc:SETTINGS>
  </fc:APPLICATION>
</fc:FIRMWARE-CONFIG>